Frequenzen des CB-Funks weltweit

Country	Band mtr	Bandwidth	Ch	Mode	Power (watts)	Antenna system 	
Italy	11	26.965-27.405	40	FM/AM	5	vert.	
U.S.A.	11	26.965-27.405	40	AM/USB/LSB	4 AM 12 SSB	vert. / horiz.	
Brasil	11	26.965-27.605	60	AM/USB/LSB	4 AM 12 SSB	vert. / horiz.	
Argentina	11	26.965-27.405	40	AM/USB/LSB	4 AM 12 SSB	vert. / horiz.	
Canada	11	26.965-27.405	40	!!!!	!!!!	!!!!	
Puerto Rico	11	26.965-27.405	40	AM/USB/LSB	4 AM 12 SSB	vert. / horiz.	
Germany	11	26.565-27.405	80	FM/AM
AM=ch. 4-15
FM=ch. 1-40	4	vert. / horiz. < 10 W ERP	
France	11	26.965-27.405	40	FM/AM/USB	1 FM-AM 4 USB	vert. / horiz. < 6db Gain	
Switerland	11	26.965 - 27.405	40	FM/AM/USB/LSB	4 FM-SSB1 AM		
Belgium	11	26.965-27.405	40	AM/FM 
- AM=22ch 
- FM= 40ch	0,5 AM / 5 FM	vert. / horiz.
< 3db Gain	
Holland	11	26.965-27.405	40	FM	4	vert. / horiz.	
Norway	11	26.965-27.405	40	AM/FM	4	vert.	
Sweden	11	26.960-27.410	40	AM/FM
AM=ch. 1-23
FM=ch. 1-40	3.5 AM 
4 FM	vert.	
Japan	11	26.968-27.144	8	!!!!	0,5	vert.	
England	11	26.965-27.405
27.60125-27.99125	40	FM 	4	vert	
Ireland	11	26.965-27.991	??	FM/AM/USB/LSB	4	vert. / horiz	
Spain	11	26.965-27.405	40	FM/AM/USB/LSB	1 FM-AM 
4 SSB	vert.	
Portugal	11	26.965-27.405	40	FM(AM+SSB with licence)	5	vert.	
Austria	11	26.965-27.405	40	FM	4	vert.	
South Africa	11	27.185-27.275	9	AM/USB/LSB	4 AM 
12 SSB	vert. 
Ødb Gain	
New Zealand	11	26.330-26.770	40	AM/USB/LSB	4 AM / 12 SSB	vert. / horiz.	
Australia	11
70cm	26.965-27.405
476.425-477.400	40
40	FM/AM/USB/LSB
FM/DSB/USB/LSB	12
5 FM / 4 DSB / 12 SSB	vert. / horiz	
Denmark	11	26.965-27.405	40	FM	4	vert. / horiz.	
Finland	11	26.965-27.405	40	FM	4	vert. / horiz.	
Namibia	11	27.185-27.295	9	AM/USB/LSB	4 AM / 12 SSB	vert. 
Ødb Gain	
Guatemala	11	26.965-27.405	40	!!!!	!!!!	!!!!	
Scotland	11	26.965-27.405
27.60125-27.99125	40	FM	4	vert.	
Wales	11	26.965-27.405
27.60125-27.99125	40	FM	4	vert.	
Guadeloupe	11	26.965-27.405	40	AM	4	vert.	
Slovenia	11	26.965-27.405	40	FM/AM	5	vert	
Czech Republic	11	26.965-27.405	40	FM/AM 
AM= Ch. 1-10	4 FM / 1 AM	vert.	

Switzerland:	RTTY AMTOR SSTV Pactor Packet Radio Channel is free but most use freq 27.235 27.245 FM Call Channel 9AM 16USB 40FM 
A CallsignChaos is not Possible in Switzerland All Peoples must have a Callsign and a Packet Callsign by a word. Packet Callsign was systematic In Zuerich we have Packet Callsign from HER200-HER299 in Bern is the Callsign HEF200-HEF999 ect The Voice Callsign was regulated in Bern have ending 62 in Zuerich we have ending 79 Switzerland have the best organized CB in Europe. 
70CM with 10Miliwatt's 933+934MHZ with 5 Watt's 
Sweden:	channel 24 is used for USB/LSB with a maximum of 12 Watts PEP
Germany:	Paket Radio allowed on